See the instructions for correct funtionality of the Bluetooth coder.





DC INPUT :6V-12V

OPERATING VOLTAGE : 1.8V-5.5V

DC OUTPUT : 5V/40mA per pin

FLASH MEMORY : 32kB

EEPROM MEMORY : 1kB

RAM : 2kB



S3 Engineering Lanka (Pvt). Ltd



Model No : BC-555

Bluetooth Coder







SN :

**MADE IN SRILANKA**