

External relay extender

Model No : ERE5V2





INPUT : 5V 500mA

OPERATIONAL RANGE : 10A 250VAC 10A 125VAC

10A 30VDC 10A 28VDC

S3 Engineering Lanka (Pvt) Ltd.



|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| NO  1 | COM  1 | NC  1 | NO  2 | COM 2 | NC  2 |

**Made in Sri Lanka**